# ACTION ALERT

PART # \_SF5005\_

CONCERN **\_Lead Chamfer of threads oversize\_**

Keep lead chamfers of thread to a minimum, especially on inside

of cup.

**Name: Steve Reckamp Date: 7/12/13**